# This is a Revit shared parameter file.
# Do not edit manually.
*META	VERSION	MINVERSION
META	2	1
*GROUP	ID	NAME
GROUP	1	01_GENERAL
GROUP	2	02_APPEARANCE
GROUP	3	03_PROTECTION
GROUP	4	04_LIGHT_SOURCE
GROUP	5	05_LIGHT_QUALITY
GROUP	6	06_OPTICS
GROUP	7	07_PERFORMANCE
GROUP	8	08_CONTROL
GROUP	9	09_ELECTRICAL
GROUP	10	10_DIMENSIONS
GROUP	11	11_LIFETIME
GROUP	12	12_CIRCUIT_LOADING
GROUP	13	13_CONNECTION
GROUP	14	14_CLASSIFICATION
GROUP	15	15_SUSTAINABILITY
*PARAM	GUID	NAME	DATATYPE	DATACATEGORY	GROUP	VISIBLE	DESCRIPTION	USERMODIFIABLE	HIDEWHENNOVALUE
PARAM	99e88404-aee0-425c-8058-7a61486bdffb	Length, mm	TEXT		10	1		1	0
PARAM	f9433605-4445-4855-8d04-0a2bd754cfa9	GWP-Total A1-A3 kgCO2e	TEXT		15	1		1	0
PARAM	b7425007-4619-47d0-b186-9c6c52a2d222	Voltage, V	TEXT		9	1		1	0
PARAM	6f4ee20e-4f48-4dc6-95d3-172eaf1288cd	Connection method Cable gland plastic with cable_1SPC	YESNO		13	1		1	0
PARAM	bb7b7e14-0be6-4eb0-8bdc-11ca22bc9aff	Height, mm	TEXT		10	1		1	0
PARAM	2c67a814-3422-46dc-8047-20d0239cde63	UGR	TEXT		6	1		1	0
PARAM	65aa141b-9d7a-4feb-90f4-0672916046d6	Colour temperature 5000K_850	YESNO		5	1		1	0
PARAM	3117a91d-cc64-42b8-a3e9-59575eff2cca	Control method Casambi Sensor PIR High Bay_CSHBW65	YESNO		8	1		1	0
PARAM	0784ab27-4c51-43b0-8e34-075a8739a30e	Maximum quantity of luminaires per circuit breakers B10	TEXT		12	1		1	0
PARAM	04b17f2a-87df-4c8f-85a1-9aa82c422694	Colour of luminaire frame	TEXT		2	1		1	0
PARAM	31f3bd2a-132d-476a-a94a-e23636882644	End cap material	TEXT		2	1		1	0
PARAM	874cc92e-3d72-4aab-86f6-3c7f3c1db1c7	Connection method One quick connector_1QAN	YESNO		13	1		1	0
PARAM	1b4d8e32-057d-4041-8b5d-8529b302b350	Optics	TEXT		6	1		1	0
PARAM	7219a233-6b6c-46ea-b9da-e85f6c7e3f9b	Enclosure class	TEXT		3	1		1	0
PARAM	12f6f233-530f-4b7a-acaf-8806914f75ec	Diameter, mm	TEXT		10	1		1	0
PARAM	b5bb1d42-0b23-45c3-93b8-e27ef9d17048	Control method on-off_OF	YESNO		8	1		1	0
PARAM	c0b25442-6d7e-4583-856c-30854cef22f7	MC National Classification Group	TEXT		14	1		1	0
PARAM	bee2094a-0a82-4513-bb00-f66c100fdd52	Enclosure class_IP65	YESNO		3	1		1	0
PARAM	79214c4d-8c40-4b42-87c7-4acb546befec	Type code	TEXT		1	1		1	0
PARAM	6479dd4e-994b-4613-a64d-da0557419050	MC National Classification Abbreviation	TEXT		14	1		1	0
PARAM	1b537954-a5be-4b71-992f-1894fa7ac1b9	Enclosure class_IP44	YESNO		3	1		1	0
PARAM	8607ca5e-1ea4-4b7b-af64-1c303279afa0	Connection method Cable gland plastic with cable quick connector without cable_1SAN	YESNO		13	1		1	0
PARAM	ba60a35f-ec68-4050-bb2b-ab620e1a75a4	Maximum quantity of luminaires per circuit breakers B20	TEXT		12	1		1	0
PARAM	12faa062-5991-4e24-90c8-753e866e9810	Impact resistance class, IK	TEXT		3	1		1	0
PARAM	1f046966-3ea1-49c8-b799-a2958cf5a961	Maximum quantity of luminaires per circuit breakers C20	TEXT		12	1		1	0
PARAM	4dfbb567-98db-4f7d-bf62-c97692b44b93	Power_Factor	TEXT		7	1		1	0
PARAM	6f06ea69-150d-4763-9ac9-1c3438b2234c	Colour temperature	TEXT		5	1		1	0
PARAM	9136196b-7880-4b68-8e3b-f62f2aecb309	MacAdams, SDCM	TEXT		5	1		1	0
PARAM	11c2c86c-46f3-4d22-9dc8-65ed666e6581	MC National Classification Code	TEXT		14	1		1	0
PARAM	c782fb71-e959-4c88-adc2-f09bf3c91130	Life time, years	TEXT		11	1		1	0
PARAM	3dc0d674-b1b6-4c6b-95b9-2ca5b40096fd	Control method DALI_DA	YESNO		8	1		1	0
PARAM	94dc4a76-e741-4420-ad4b-47fdfb718271	Maximum quantity of luminaires per circuit breakers B16	TEXT		12	1		1	0
PARAM	af6e137f-6832-4d23-9055-6ac7179f3734	MC National Classification Description	TEXT		14	1		1	0
PARAM	26cec280-55d1-4701-a44c-49c98378579b	Connection type	TEXT		13	1		1	0
PARAM	5cf13c8c-8226-4981-a8df-c30c3511dfd5	Model	TEXT		1	1		1	0
PARAM	73ed4f8c-a8a5-486a-9834-5ac8aaf7d004	Light source protection material	TEXT		4	1		1	0
PARAM	b2fc6299-2aff-4cbf-9ca6-eed985e5bb57	Power, W	TEXT		7	1		1	0
PARAM	a6af02a0-2ad1-483f-bdd2-d563f9e3280e	Width, mm	TEXT		10	1		1	0
PARAM	a65660a4-1dac-4328-a846-257954ee9961	Approved for continuation of branch circuit	TEXT		13	1		1	0
PARAM	ddd69fab-c145-4fc9-a2bd-ffb3ec941197	Number of DALI adresses	TEXT		9	1		1	0
PARAM	092497b7-97d1-46c7-9690-708a866664c4	Maximum quantity of luminaires per circuit breakers C10	TEXT		12	1		1	0
PARAM	b68a97b9-d77b-47ac-8db6-52bbca056d61	Lifetime L90B50	TEXT		11	1		1	0
PARAM	102e88c1-0648-4eee-9768-9b735c9aeb5a	Control method NLC Sensor Casambi Sensor PIR Low Bay_CSLBW65	YESNO		8	1		1	0
PARAM	f3421cc3-6c4a-4f89-989c-41e3aae848a7	Colour temperature 3000K_830	YESNO		5	1		1	0
PARAM	7679bdc4-2e77-4c47-aa09-add88733aeff	Light source	TEXT		4	1		1	0
PARAM	157164d1-2fba-418d-ab01-9d0216fbd935	Mass, kg	TEXT		10	1		1	0
PARAM	ce1fa1d4-fd84-4a15-b42e-c63bde92b018	Luminous flux, lm	TEXT		7	1		1	0
PARAM	65f56edb-dbfc-49b2-9e5d-8767b65f9891	Control method	TEXT		8	1		1	0
PARAM	2221a5db-6ffe-4602-865c-35ab59ea70a6	Colour temperature 4000K_840	YESNO		5	1		1	0
PARAM	30b7dfdc-ad33-4e96-9a49-4f0a31cbb2e9	GWP-Fossil A1-A3 kgCO2e	TEXT		15	1		1	0
PARAM	ff6eabdd-3d4d-4648-af25-c9a426b19d8a	Electrical number	TEXT		9	1		1	0
PARAM	7328f9e0-0ddb-4865-a504-6f33e48d0554	Connection method Two quick connector without cable_2QAN	YESNO		13	1		1	0
PARAM	4db4c5e3-bde2-4f22-9c98-a66e769391be	Colour rendering index	TEXT		5	1		1	0
PARAM	745df3e7-197e-4369-aee9-817b5c8fdc47	Order code	TEXT		1	1		1	0
PARAM	d95317ed-2960-4c37-9741-c6e80b92931d	Apparent Load	TEXT		7	1		1	0
PARAM	965fe2ed-8afc-45b6-807a-52202ca2a11a	Maximum quantity of luminaires per circuit breakers C16	TEXT		12	1		1	0
PARAM	4481d7f4-1abd-4bc5-a695-5b84aca1b8a1	Led-Driver current mA	TEXT		9	1		1	0
PARAM	53214ef6-ee22-456c-acb8-283b3200d306	Manufacturer	TEXT		1	1		1	0
PARAM	209017f7-9cef-4ba6-b086-bd7662ffda4a	LED Type	TEXT		4	1		1	0
PARAM	bbe673f9-6ec0-423c-83ac-45dbc0c40c72	Control method NLC Sensor PIR High Bay_NLPHBW65	YESNO		8	1		1	0
PARAM	bee567ff-4e12-4fad-b4a6-e8bea08cf67a	MC National Classification Subgroup	TEXT		14	1		1	0
PARAM	12a2fcff-f4e5-4582-bcc8-0650929cddd6	Control method NLC Sensor PIR Low Bay _NPLBW65	YESNO		8	1		1	0
